**Requirement Specification for Weapon lubricant**

1. **Requirements**

**1.1. Description and definitions**

The requirement specification, cf. section 1.4, describes all the requirements for the acquisition and consists of six columns with the following information:

|  |  |
| --- | --- |
| "#" | ID number |
| "Requirement" | Requirement description |
| "Classification" | The classification of the requirement as further described in section 1.3 |
| "DALO remarks" | Further information regarding the requirement |
| "Requirement compliance" | The tenderer's indication of compliance (YES or NO) |
| "Tender description" | Requirements regarding the tenderer's compliance description  |

**1.2. Classification**

All requirements are mandatory requirements (SHALL) and shall be fulfilled by the tenderer. If just one of the mandatory requirements is not fulfilled, the tenderer's tender will not be taken into further consideration.

**1.3. Requirement and response sheet**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **#** | **Requirement** | **Classification** | **DALO remarks** | **To be filled out be the tenderer** |
| **Requirement compliance** | **Tenderer's description** |
| **YES** | **NO** |
| **1** | The S-758 products shall meet all the requirements of MIL-SPEC: “MIL-PRF-63460E - Performance specification – Cleaner, lubricant and preservative for weapons and weapons systems” or equivalent. | SHALL | Specifications which have been accepted under NATO Code Number S-758 may be considered equivalent.Acceptance on the associated Qualified Products List (e.g. QPL-63460), an official valid certificate or documented test results for the current formulation of the product are examples of acceptable forms of documentation for compliance with this requirement. |  |  |  |
| **2** | The Supplier shall comply with any legal requirements for the marking of containers. | SHALL |  |  |  |  |
| **3** | The Supplier shall comply with regulation (EC) No 1272/2008 of the European Parliament and of the Council, of 16 December 2008, on classification, labelling and packaging of substances and mixtures (CLP) including all following amendments of the regulation and undertake the obligations of the Supplier described therein regardless of whether the Supplier is in fact based inside or outside the European Union. | SHALL |  |  |  |  |
| **4** | The labelling necessitated by Requirement ID 2 shall be in Danish language. | SHALL |  |  |  |  |
| **5** | The Supplier shall comply with Regulation (EC) No 1907/2006 OF THE EUROPEAN PARLIAMENT AND OF THE COUNCIL of 18 December 2006, concerning the Registration, Evaluation, Authorisation and Restriction of Chemicals (REACH) including all following amendments of the regulation and undertake the obligations of the Supplier described therein regardless of whether the Supplier is in fact based inside or outside the European Union. | SHALL |  |  |  |  |
| **6** | For all offered products, the Supplier shall provide a Safety Data Sheet compliant with the requirements set out by Commission Regulation (EU) 2015/830 of 28 May 2015, amending Regulation (EC) No 1907/2006 of the European Parliament and of the Council on the Registration, Evaluation, Authorisation and Restriction of Chemicals (REACH). | SHALL | The Supplier shall enclose the Safety Data Sheets. |  |  |  |
| **7** | The Safety Data Sheets necessitated by Requirement ID 5 shall be written in Danish or English language.Danish language is strongly preferred. | SHALL |  |  |  |  |
| **8** | The offered products shall not contain any hazardous substance or mixture, which in accordance with the regulation (EC) No. 1272/2008 are classified as:* carcinogenic, categories 1A, 1B or 2
* mutagenic, categories 1A, 1B or 2
* reproduction toxic, categories 1A or 1B

persistent, bioaccumulative and toxic (PBT) or very persistent and very bioaccumulative (vPvB) substances | SHALL |  |  |  |  |
| **9** | We will need the below mentioned sizes and quantities after the above mentioned instructions:20 ml5500 ea | SHALL |  |  |  |  |
| **10** | We will need the below mentioned sizes and quantities after the above mentioned instructions:120 ml1750 ea | SHALL |  |  |  |  |
| **11** | We will need the below mentioned sizes and quantities after the above mentioned instructions:474 ml1400 ea | SHALL |  |  |  |  |
| **12** | We will need the below mentioned sizes and quantities after the above mentioned instructions:1 L150 ea | SHALL |  |  |  |  |
| **13** | We will need the below mentioned sizes and quantities after the above mentioned instructions:5 L100 ea | SHALL |  |  |  |  |